**6.16-Bit subtraction for 8085**

